30 July 2026
CSCN Meeting
TIF 118 (Update CSCN-Administered Guidelines for Thousands-Block Pooling)
Conference Call

Participants:	Alex Wearn Tremblay - COMsolve Inc. (CNA)
David Comrie - COMsolve Inc. (CNA)
Fiona Clegg - COMsolve Inc. (CNA)
Kelly T. Walsh - COMsolve Inc. (CNA)
Natalie Ann Lessard - COMsolve Inc. (CNA)
Stephen Walsh - COMsolve Inc. (CNA)
Francois Dalton - City West
Chantale Neapole - CLNPC
Rodger McNabb - CLNPC
Bill Barsley - CNAC
Gary Jessop - CNAC
Glenn Pilley - CNAC
Ed Antecol - COMsolve Inc.
Alexander Pittman - CRTC staff
Étienne Robelin - CRTC staff
Sage Wiese - CTA
Kim Brown - Eastlink
Michael Adesina - Freedom Mobile
Andrew Hew - Rogers
Michael Studniberg - Rogers
Bruce Uy - Rogers West
Aditi Sharma - Sasktel
Diane Dolan - Teksavvy
Ajit Arya - TELUS
Akshay Chaturvedi - TELUS
Beth Connell - TELUS
Marlo Gelito - TELUS
Rick Cousineau - TELUS
James Sewell - Westman Communications


Welcome:

Kelly Walsh, as CSCN Chair, welcomed the attendees.

David Comrie, as CSCN Secretary, reviewed the list of participants.

Action Item Review:

1) None

Discussion:

The group resumed review of CNCO316C.



CNCO316C - CNA contribution - TIF 118 - Draft Part 1B for a Pooled CO Code or Block request (incl. in-meeting changes)

Agreement was reached to accept CNCO316C as the accepted Part 1B to be used for interim use. 

Action Item: The CSCN Secretary will post the modified version of CNCO316C as CNCO316D and be posted on the CSCN Drafts page. A clean version of the form will be posted on the CNA website with a note that it has received interim approval from the CSCN. (Completed)

The Chair thanked everyone for participating.

Summary of Agreements Reached:

1) Agreement was reached to accept CNCO316C as the accepted Part 1B to be used for interim use. 

Summary of Action Items:

1) The CSCN Secretary will post the modified version of CNCO316C as CNCO316D and be posted on the CSCN Drafts page. A clean version of the form will be posted on the CNA website with a note that it has received interim approval from the CSCN. (Completed)
Attachment:

See text above for the attachment.
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CRTC INTERCONNECTION STEERING COMMITTEE
CONTRIBUTION FORM:
Working Group:       CSCN                        Date of Submission:  2026-02-23
Contribution #:  316C
TIF #:    118                                  File ID:  CNCO316C
Task Title:  Update CSCN-Administered Guidelines for Thousands-Block Pooling
Related to Task(s) ID:  117, 119, 120, 125, 126
Contributor:
            Name:		CNA
            Company:	CNA
            Address:
            Tel:
            Fax:
            E-mail:	david.comrie@cnac.ca
Distribution to:	CSCN
Subject:	Draft Part 1B form for Pooled CO Code and Block requests






NPAC Thousands-Block Data - Part 1B

Revised: January 21, 2025

NPAC Block Holder Data

Submit one form per Thousands-Block.

Block Creation/Activation Request: ☐		Modification Request: ☐

This form should be filled out by applicants who are activating/modifying a new Block where they are not the Code Holder, or where they are the Code Holder but the Block is being allocated to a different LRN.

For Block Creations using NPAC Activation, fill section A and optionally section B.
For activations using SOA Activation, only fill in section A.

Modifications through the CNA can only be done if the application (Part 1A and Part 1B) is submitted 19 calendar days before the NPAC Block Effective Date. Changes on/after the NPAC Block Effective Date must be done by the Block Holder using their SOA or LTI.



Section A:



CNA Contact 

Phone: 613-702-0016

E-Mail: COCodeApps@cnac.ca 



Block Applicant 

Company Name: Click here to enter text.

Contact Name: Click here to enter text.

Address: Click here to enter text.

City:  Click here to enter text.  State: Click here to enter text.  Postal Code: Click here to enter text.

Phone: Click here to enter text. 	

E-Mail: Click here to enter text.  	

Service Provider NPAC SOA SPID[footnoteRef:1]:              Click here to enter text. [1:  The Service Provider ID of the Thousands-Block Holder.  The SPID shall be a valid SPID in the NPAC system. If your company does not have a SPID, please call the NPAC Help Desk for assistance.] 


LRN[footnoteRef:2]:	         Click here to enter text. [2:  A Location Routing Number is a 10-digit number, in the format NPA-NXX-XXXX, that uniquely identifies a Switching Entity/POI.  The NPA-NXX portion of the LRN is used to route calls. ] 




Block (1K) Range[footnoteRef:3]:           Click here to enter text. [3:  The Thousands-Block shall consist of NPA-NXX and the first digit of the 1K block in the format NPA-NXX-X.] 


If Block Applicant is seeking to activate a Thousands-Block, Pooling Administratorthe CNA will fill in the information for the assigned block in the field belowabove. Otherwise for a Modification Request or an Intra SP Block Port Request, Block Holder must specify the Block (1K) Range.



NPAC Block Effective Date[footnoteRef:4] (YYYY-MM-DD):           Click here to enter date. [4:  Typically the NPAC Block Effective Date and the BIRRDS Block Effective Date are the same date. However, based on events in CNAS, BIRRDS or NPAC, the dates may end up different.] 


NPAC Block Effective Date must be equal to or greater than the earliest date that the NPAC shall broadcast the Thousands-Block information to all Local SMSs. If the NPAC Block Effective Date is blank or the interval too short, the CNA shall set the NPAC Block Effective Date to the earliest date that the NPAC shall broadcast the Thousands-Block information to all Local SMSs.



Is Block being allocated back to Code Holder using the same LRN? Yes☐ No ☐

If “Yes”, the CNA will not send the Part 1B to the NPAC. If “No”, the CNA will forward the Part 1B to the NPAC.



Activation of Block Range (Must Select only One)

NPAC Activation ☐	

SOA Activation ☐

If “NPAC” is selected the NPAC shall activate the Thousands-Block range. If “SOA” is selected it shall be the responsibility of the Service Provider (SP) to activate the Thousands-Block range via their Service Order Administration (SOA) system.




Section B:

Block Applicant to provide this data ONLY if NPAC Activation is selected. 



Whenever a Destination Point Code (DPC) value is specified, a Services Subsystem Number (SSN) value likewise must be provided (and vice versa). 



The format of the DPC shall consist of three 3-digit segments (Network Identification-Network Cluster-Cluster Member) based on the ANSI standard where each segment must be between 000 and 255.  Example: 0-0-0 to 255-255-255.  Signaling Services Subsystem Number (SSN) shall be a value between 0 and 255.



Class DPC[footnoteRef:5]: Click here to enter text. [5:  Customer Local Area Signaling Services Destination Point Code for 10-digit GTT for CLASS features for the 1K block.] 


Class SSN[footnoteRef:6]: Click here to enter text. [6:  Customer Local Area Signaling Services Subsystem Number for the 1K block.] 


LIDB DPC[footnoteRef:7]: Click here to enter text. [7:  Line Information Database Destination Point Code for 10-digit GTT for LIDB features for the 1K block.] 


LIDB SSN[footnoteRef:8]: Click here to enter text. [8:  Line information Database Subsystem Number for the 1K block.] 


CNAM DPC[footnoteRef:9]: Click here to enter text. [9:  Calling Name Delivery Destination Point Code for 10-digit GTT for CNAM features for the 1K block.] 


CNAM SSN[footnoteRef:10]: Click here to enter text. [10:  Calling Name Delivery Subsystem Number for the 1K block.] 


ISVM DPC[footnoteRef:11]: Click here to enter text. [11:  Inter-Switch Voice Mail Destination Point Code for 10-digit GTT for ISVM features for the 1K block.] 


ISVM SSN[footnoteRef:12]: Click here to enter text. [12:  Inter-Switch Voice Mail Services Subsystem Number for the 1K block.] 


WSMSC DPC[footnoteRef:13]: Click here to enter text. [13:  Wireless Short Message Service Center Destination Point Code for 10-digit GTT for WSMSC features.  This field is only required if the Service Provider (SP) supports WSMSC data.] 


WSMSC SSN[footnoteRef:14]: Click here to enter text. [14:  Wireless Short Message Service Center Subsystem Number for the 1K block.  This field is only required if the Service Provider (SP) supports WSMSC data.] 





Section C:

This section is completed by the NPAC after processing. NPAC is to Activate/Modify/Port the Block (1K), as indicated on this form. When the Block (1K) Activation/Modification is complete, NPAC sends a copy of the completed form to the CNA.

Block (1K) Request Complete: Yes ☐	No ☐

Complete Date: Click here to enter a date.

Complete Time (HH/MM): Click here to enter text.

NPAC Personnel performing change: Click here to enter text.



Block Holder sent Completed Form: Yes ☐	No ☐

Mailed Date: Click here to enter a date.

Mailed Time (HH/MM): Click here to enter text. 

Contact Name: Click here to enter text.

Pooling Administrator sent Completed Form: Yes ☐	No ☐

Mailed Date:  Click here to enter a date.

Mailed Time (HH/MM): Click here to enter text. 

Contact Name: Click here to enter text.



Remarks: Click here to enter text.
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