Central Office Code Assignment Guidelines (COCAG)

Central Office Code (NXX) Assignment Request - Part 2, Form 8

**Revised: September 5, 2014**

Following are Switch Homing Arrangement (SHA) data requirements for the iconectiv BIRRDS database. Section 1.6.1of the COCAG/TBPAG Forms Part 2 Job Aid may be referenced for assistance in completing this form.

**New SHA (with same 11 CLLI™[[1]](#footnote-1) as another SHA)** All items are required unless otherwise noted.

**Data change** Items 1-4 are required, as are the appropriate element(s) to be changed.

**Disconnect** Only items 1-4 should be provided.

1. **SWITCH** Click here to enter text.

Eleven character CLLI[[2]](#footnote-2)™ code that identifies the switching entity/POI. For CO Code assignments, this is the switching entity/POI that will originate/terminate calls from/to the assigned CO Code.

1. **SHA IND** Click here to enter text.

Switch Homing Arrangement Indicator (01-99).

1. **STATUS** Click here to enter text.

E = new entity/POI, M = change to supporting data, D = disconnect.

1. **EFF DATE** Click here to enter a date.

Date a new switching entity/POI can be routed to, date supporting data change will be effective or, date of disconnect (mm/dd/yy).

1. **Homing Arrangements**

As may be applicable, enter the appropriate eleven character SWITCH (e.g. CLLI™) to which the switching entity/POI may home to for various feature group capabilities, signaling, etc.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ORIGINATING:** |  | **TERMINATING:** |  | **ADDITIONAL:** |  |
| FG B TDM: | Click here to enter text. | FG B TDM: | Click here to enter text. |  |  |
| FG C TDM: | Click here to enter text. | FG C TDM: | Click here to enter text. |  |  |
| FG D TDM: | Click here to enter text. | FG D TDM: | Click here to enter text. |  |  |
| OS TDM: | Click here to enter text. | OS TDM: | Click here to enter text. |  |  |
| FG B INT: | Click here to enter text. | FG B INT: | Click here to enter text. |  |  |
| FG C INT: | Click here to enter text. | FG C INT: | Click here to enter text. | ISDN FS OFC: | Click here to enter text. |
| FG D INT: | Click here to enter text. | FG D INT: | Click here to enter text. |  |  |
| LOCAL TDM: | Click here to enter text. | LOCAL TDM: | Click here to enter text. |  |  |
| INTRA TDM: | Click here to enter text. | INTRA TDM: | Click here to enter text. |  |  |
| CS DATA TDM: | Click here to enter text. | CS DATA TDM: | Click here to enter text. |  |  |

1. CLLI™ is a trademark of Telcordia Technologies, Inc. dba iconectiv. [↑](#footnote-ref-1)
2. [↑](#footnote-ref-2)