27 July 2026
CSCN Meeting
TIF 118 (Update CSCN-Administered Guidelines for Thousands-Block Pooling)
Conference Call

Participants:	Alex Wearn Tremblay - COMsolve Inc. (CNA)
David Comrie - COMsolve Inc. (CNA)
Fiona Clegg - COMsolve Inc. (CNA)
Kelly T. Walsh - COMsolve Inc. (CNA)
Stephen Walsh - COMsolve Inc. (CNA)
Isaac Hayford - Access Communications
Joey-Lynn Abdulkader - Bell Canada
Francois Dalton - City West
Paul Fleming - City West
Chantale Neapole - CLNPC
Rodger McNabb - CLNPC
Bill Barsley - CNAC
Glenn Pilley - CNAC
Ed Antecol - COMsolve Inc.
Alexander Pittman - CRTC staff
Étienne Robelin - CRTC staff
Sage Wiese - CTA
Kim Brown - Eastlink
Michael Adesina - Freedom Mobile
Vince Yelle - Groupe Maskatel
Marcel Champagne - Neustar/Transunion
Andrew Hew - Rogers
Jennifer Mack - Rogers
Michael Studniberg - Rogers
Bruce Uy - Rogers West
Aditi Sharma - Sasktel
Lucie Lang - Sasktel
Bob Bruce - Syniverse
Diane Dolan - Teksavvy
James Sewell - Westman Communications


Welcome:

Kelly Walsh, as CSCN Chair, welcomed the attendees.

David Comrie, as CSCN Secretary, reviewed the list of participants.

Action Item Review:

1) None

Discussion:


Kelly Walsh noted that there are versions of the CO Code Part 1A and Part 1B which have been posted on the CNA website for a while. They have been used by the CNA recently to facilitate the assignment of Thousands Blocks. The goal of this meeting is to review the current versions of the forms to get CSCN approval to use the forms on an interim basis.

Kelly Walsh presented CNCO315B.



CNCO315B - CSCN contribution - TIF 118 - Draft Part 1A for a Pooled CO Code or Block request (incl. in-meeting changes)

Ed Antecol asked if carriers transferring from one operating arm to another with different OCNs would need to complete the Part 1A. Kelly Walsh noted that they would.

Kelly Walsh noted that if you need to take a replenishment CO Code because there are not enough available Blocks, then you have to take at least 1 Block from the new CO Code but it does not have to be Block 0. It could be any of the blocks in the CO Code.

Ed Antecol noted that if you are forced to take an AP Block and someone else is not doing something to make it useful, you are either going to have to write the CNA or CRTC to say that you were forced to take this Block but the Carrier for the CO Code has not done the necessary work to get this done. Kelly Walsh noted that the CNA is going to get a failure when submitting the 1B if the CO Code has not been added to the NPAC.

Sage Wiese asked why you would assign a Block with an AP status if it runs the risk of causing issues. Ed Antecol noted that it usually resolves itself in time and this is the same process that is in place in the US. It only rarely causes an issue.

Ed Antecol suggested that requiring companies to take AP Blocks if that’s the only Block left could be revisited if it proves to be a problem.

Agreement was reached to accept CNCO315B as the new Part 1A form for interim use.

Action Item: The CSCN Secretary will post the modified version of CNCO315B as CNCO315C on the CSCN Drafts page. A clean version of the form will be posted on the CO Code Guidelines page with “Interim, CSCN approved” indicated. (Completed)

Kelly Walsh presented CNCO316C.




CNCO316C - CNA contribution - TIF 118 - Draft Part 1B for a Pooled CO Code or Block request (incl. in-meeting changes)

Fiona Clegg noted that in a future meeting, we also need to consider section 4.2.2 of the Canadian TBCOCAG.

Action Item: David Comrie will send out a meeting invitation for TIF 118 Thursday, 30 July 2026 from 12:30 to 2:00pm ET.

The Chair thanked everyone for participating.

Summary of Agreements Reached:

1) Agreement was reached to accept CNCO315B as the new Part 1A form for interim use.
Summary of Action Items:

1) The CSCN Secretary will post the modified version of CNCO315B as CNCO315C on the CSCN Drafts page. A clean version of the form will be posted on the CO Code Guidelines page with “Interim, CSCN approved” indicated. (Completed)

2) David Comrie will send out a meeting invitation for TIF 118 Thursday, 30 July 2026 from 12:30 to 2:00pm ET.
Attachment:

See text above for the attachment.
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	Canadian Central Office Code (NXX) Assignment Guidelines Part 1A – Thousands-Block Assignment, Information Change, or Disconnect: CSCN Approval Date 18 December 2024


CRTC INTERCONNECTION STEERING COMMITTEE
CONTRIBUTION FORM:
Working Group:       CSCN                        Date of Submission:  2026-02-12
Contribution #:  315B
TIF #:    118                                  File ID:  CNCO315B
Task Title:  Update CSCN-Administered Guidelines for Thousands-Block Pooling
Related to Task(s) ID:  117, 119, 120, 125, 126
Contributor:
            Name:		CSCN Secretary
            Company:	CSCN
            Address:
            Tel:
            Fax:
            E-mail:	Secretary-CSCN@cnac.ca
Distribution to:	CSCN
Subject:	Draft Part 1A form for Pooled CO Code and Block requests



Part 1A – Application For a Pooled CO Code and Thousands-Block Assignments, Information Change, or the Return of Thousands-Blocks



This Part 1A form is to be used by an Applicant for:

(i) a Pooled CO Code Assignment with one or more Thousands-Blocks;

(ii) Thousands-Block Assignments from an existing Exchange Area Pool,

(iii) An information change related to Thousands-Blocks, 

(iv) Transfer related to Thousands-Blocks, or

(v) the Return of Thousands-Block(s). 



Electronically submit the completed form to the Canadian Numbering Administrator (CNA). As of the date of issue of this form, the CNA contact information is:

Telephone: (+1) 613 702-0016 

E-mail: COCodeApps@cnac.ca 

Postal address: 880 Taylor Creek Dr, Rm 102, Orleans, ON K4A 0Z9 



See http://www.cnac.ca/about/contact_us.htm for updates to CNA contact information.



I hereby certify that the following information is true and accurate to the best of my knowledge and that this application has been prepared in accordance with the currently applicable version of the Canadian Thousands-Block and Central Office Code (NXX) Assignment Guidelines (“C-TBCOCAG”).





	<No signature required if filed via CNA Secure Portal>



____________________________________________________________

Signature of Authorized Representative of Code Applicant or Code Holder



___________________________________________________________

Name of Authorized Representative of Code Applicant or Code Holder



____________________________________________________________

Title



____________________________________________________________

Date








1.  General Application Information



Contact Name: Click here to enter text.

Entity OCN: Click here to enter text.

Entity Name: Click here to enter text.

Address: Click here to enter text.

City: Click here to enter text. 

Province: Click here to enter text. 

Postal Code: Click here to enter text.

Phone: Click here to enter text.	

E-Mail: Click here to enter text.

Date of Application[footnoteRef:1]: Click here to enter a date.   [1:  Acknowledgment and indication of disposition of this application shall be provided to applicant within fourteen calendar days from the date of receipt of this application.  An incomplete form may result in delays in processing this request.] 




Type of Application (Check one):

☐ New Pooled Geographic Number Resource Assignment (complete section 2)

☐ Information Update for assigned Pooled Geographic Number Resource (complete section 3)

☐ Transfer Thousands-Blocks (complete section 4)

☐ Return of Thousands-Blocks (complete section 5)



2.	Pooled CO Code/Block Application





a) Requested Effective Date[footnoteRef:2] (yyyy-mm-dd): Click here to enter a date. [2:  Please ensure that the Central Office (CO) Code (NPA-NXX) of the LRN to be associated with this Thousands-Block(s) is/will be active in the PSTN prior to the effective date of the Thousands-Block(s).  For a Thousands-Block assignment not involving a pool replenishment request, the requested Effective Date shall be no earlier than 40 days and no later than 6 months after the date of application. For a Pooled CO Code assignment, the requested Effective Date shall be no earlier than 66 days and no later than 6 months after the date of application.  ] 




b) Requested Expedited CNA Treatment by CNA? See section <TBD>6.2.2 of Guidelines 
Yes ☐



By selecting Yes, I acknowledge that I am requesting the earliest possible Effective Date the Administrator can grant. Please note that this only applies to a reduction in the Administrator’s processing time, however the request will still be processed in the order received.



(Section 2.b is not applicable where a shorter interval is requested requiring approval of an Emergency Notification by CRTC staff)



2.1	Declarations



In accordance with Telecom Regulatory Policy CRTC 2024-26, an attestation is required from applicants and their authorized representative(s) requesting geographic NANP numbers. I attest:



☐ the newly assigned numbers will be used only for services that require geographic NANP numbers;

☐ resources other than NANP geographic resources (such as non-geographic numbers or dummy numbers) cannot be used instead; and,

☐ the carrier does not have unused numbering resources from previous assignments that can be used instead.



2.2	Certification





Provide a traceable reference to the certification or authorization required by providing the certification type, date and reference number or provide other explanation:

 Click here to enter text.





2.3	Type of Service Provider Requesting the Thousands-Block 



a) Type of Service Provider (e.g., LEC, Wireless Carrier): Click here to enter text. 



b) Primary Type of Service Blocks to be used for (e.g., Wireline, Wireless): Click here to enter text.





2.4	Regulatory Checks 



a) Initial block(s) for Exchange Area:



Yes ☐ 	    



If requesting more than 1 Block, attach months to exhaust worksheet found here:	Appendix B - Months-to-Exhaust Certification Worksheet



b) Growth blocks within an Exchange Area: 



Yes ☐ 	If yes, attach months to exhaust worksheet found here:	Appendix B - Months-to-Exhaust Certification Worksheet 







2.5	Resource Request (Choose only one of Option A, B or C below):



Option A: Pooled CO Code to establish a new LRN



NPA Complex: Click here to enter text.



Exchange Area[footnoteRef:3]: Click here to enter text. [3:  The Exchange Area on this form and on the Appendix B worksheet shall be a tariffed Exchange Area and shall be the Exchange Area where the CO Code will be or is assigned, rather than the Exchange Area containing the Switch Identification (Switching Entity/POI) CLLI, which may be the same or different. The name of the Exchange Area is generally the same as the name of the Rate Center.] 




LATA:	888



Switch Identification (Switching Entity / POI) [footnoteRef:4],[footnoteRef:5]: Click here to enter text. [4:  This is the 11-character iconectiv® COMMON LANGUAGE® CLLITM of the Code Applicant's Switching Entity/POI (physical or virtual). (CLLI is a trademark of iconectiv LLC, and COMMON LANGUAGE is a registered trademark of iconectiv LLC).]  [5:  Please include a spreadsheet identifying Switching Entity/POI to Block mapping where more than one Switching Entity/POI is requested.] 




Preferred CO Codes (NPA-NXX): Click here to enter text.



Undesirable CO Codes (NPA-NXX): Click here to enter text.



Number of Thousands-Blocks Requested (1-10): Click here to enter text.



Thousands-Blocks to be retained from new Pooled CO Code (check below) 



		Block0

		Block1

		Block2

		Block3

		Block4

		Block5

		Block6

		Block7

		Block8

		Block9



		☐

		☐

		☐

		☐

		☐

		☐

		☐

		☐

		☐

		☐










Option B: Pooled CO Code for pool replenishment[footnoteRef:6] [6:  CNA will refuse the pool replenishment request if there are a sufficient number of Thousands-Blocks available in the Exchange Area Pool.  See Guidelines] 




If the available Thousands-Blocks in the Exchange Area Pool is sufficient to satisfy your requirements, your application for a new Pooled CO Code will be denied.  Information on Exchange Area Pools can be found here: https://cnac.ca/co_codes/co_block_status.htm



NPA Complex: Click here to enter text.



Exchange Area[footnoteRef:7]: Click here to enter text. [7:  The Exchange Area on this form and on the Appendix B worksheet shall be a tariffed Exchange Area and shall be the Exchange Area where the CO Code will be or is assigned, rather than the Exchange Area containing the Switch Identification (Switching Entity/POI) CLLI, which may be the same or different. The name of the Exchange Area is generally the same as the name of the Rate Center.] 




LATA:	888



Switch Identification (Switching Entity / POI) [footnoteRef:8],[footnoteRef:9]: Click here to enter text. [8:  This is the 11-character iconectiv® COMMON LANGUAGE® CLLITM of the Code Applicant's Switching Entity/POI (physical or virtual). (CLLI is a trademark of iconectiv LLC, and COMMON LANGUAGE is a registered trademark of iconectiv LLC).]  [9:  If any of the Blocks being requested are for a different Switching Entity/POI within the same Exchange Area then additional Part 1B forms are required for each such Block with a Switching Entity/POI that is different than the Switching Entity/POI associated with the CO Code. Also please include a spreadsheet identifying Switching Entity/POI to Block mapping.] 




Preferred CO Codes (NPA-NXX): Click here to enter text.



Undesirable CO Codes (NPA-NXX): Click here to enter text.



Number of Thousands-Blocks Requested (1-10): Click here to enter text.



Thousands-Blocks to be retained from new Pooled CO Code (check below)



		Block0

		Block1

		Block2

		Block3

		Block4

		Block5

		Block6

		Block7

		Block8

		Block9



		☐

		☐

		☐

		☐

		☐

		☐

		☐

		☐

		☐

		☐







	




Option C: Thousands-Blocks from an Exchange Area Pool:



Please consult available inventory on https://cnac.ca/co_codes/co_block_status.htm before completing the section below. Inventory is assigned first come, first served. 



		AV (Available)

		A thousands-block that is available for assignment.



		AF (Available)

		A thousands-block that is available for assignment; however, it has a future effective date.



		AP (Available)

		A thousands-block that is available for assignment; however, it is pending verification of activation in the PSTN by the LERG assignee.









NPA Complex: Click here to enter text.



Exchange Area[footnoteRef:10]: Click here to enter text. [10:  The Exchange Area on this form and on the Appendix B worksheet shall be a tariffed Exchange Area and shall be the Exchange Area where the CO Code will be or is assigned, rather than the Exchange Area containing the Switch Identification (Switching Entity/POI) CLLI, which may be the same or different. The name of the Exchange Area is generally the same as the name of the Rate Center.] 




LATA:	888



Switch Identification (Switching Entity / POI) [footnoteRef:11],[footnoteRef:12]: Click here to enter text. [11:  This is the 11-character iconectiv® COMMON LANGUAGE® CLLITM of the Code Applicant's Switching Entity/POI (physical or virtual). (CLLI is a trademark of iconectiv LLC, and COMMON LANGUAGE is a registered trademark of iconectiv LLC).]  [12:  Please include a spreadsheet identifying Switching Entity/POI to Block mapping where more than one Switching Entity/POI is requested.] 




Number of Thousands-Blocks Requested: Click here to enter text.



Preferred Thousands-Blocks (enter one NPA-NXX-X per cell. Preference order: [R1, C1], [R1 C2], [R1 C3], [R1, C4], [R1 C5], [R2 C1], [R2 C2], [R2 C3]) (enter below):



		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.



		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.



		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.



		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.





	Attach separate sheet if required.

Note: For each block requested you must include a Part 1B where you are not the Code Holder, or where you are the Code Holder but the Block is being allocated to a different LRN.








Undesirable Thousands-Blocks (format NPA-NXX-X) (enter below)





		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.



		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.



		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.

		Click here to enter text.





Attach separate sheet if required.



The CNA will flag Thousands-Blocks that are available in an Exchange Area Pool from a CO Code that is not yet confirmed active by the CO Code Holder. The box below must be checked if requesting a Thousands-Block from a CO Code that is not yet confirmed active by the CO Code Holder i.e., an Available Pending (AP) Thousands-Block.



Optional: 



☐ By selecting this checkbox, I acknowledge that I am willing to accept a Thousands-Block and explicitly understand that the underlying CO Code may not yet be activated in the PSTN and provisioned in the NPAC on the Thousands-Block effective date.





3.	Information Change (Mark all that apply) 





NPA-NXX(s) affected (if applicable):	 Click here to enter text.

NPA-NXX-X(s) affected:			 Click here to enter text.



Type of change: 		Details (provide attachment if needed):



     

☐ Switching Entity / POI:		Click here to enter text.



☐ Effective Date:			Click here to enter a date.



☐ Exchange Area:			Click here to enter text.

Provide a traceable reference to the certification or authorization required by providing the certification type, date and reference number or provide other explanation:

 Click here to enter text.

☐ LRN change prior to NPAC Block Activation:	

☐ Other:				Click here to enter text.



If changing the information for more than one Thousands-Block, attach separate sheet with details for each Thousands-Block impacted by the change.







4.	Transfer

All transfers need to include a letter from the losing OCN agreeing to the transfer of resource(s) to the gaining OCN.



NPA-NXX-X(s) affected:		 Click here to enter text.



Details of transfer[footnoteRef:13],[footnoteRef:14] [13:  The losing OCN should have ensured that all necessary Intra SP ports have been completed in the NPAC and that the Block(s) have been protected from further assignment before the transfer.]  [14:  While you can affect an OCN Change within the CNA records and BIRRDS, there are NPAC impacts that need to be addressed through the NPAC Help Desk.] 




Losing OCN: 	Click here to enter text.



Gaining OCN:	Click here to enter text.	



Requested Effective Date (yyyy-mm-dd): Click here to enter a date.



New Switching Entity / POI:	Click here to enter text.







5.	Block Return



NPA-NXX-X affected:		Click here to enter text.

Service Provider NPAC SOA SPID:	Click here to enter text.

The Effective Date will be provided by the CNA on the Part 3 confirmation form



a) Is this block Contaminated?: Yes ☐ No ☐

b) If yes, how many TNs are NOT available for assignment: Click here to enter text.

c) Have all necessary Intra SP ports been completed in the NPAC?: Yes ☐ 

d) Has this block been protected from further assignment?: Yes ☐ 

e) Does the Thousands-Block record exist in BIRRDS?: Yes ☐ No ☐



If returning more than one Thousands-Block, attach a separate sheet(s) with answers to above questions for each Thousands-Block being returned.





General Remarks: Click here to enter text.
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CRTC INTERCONNECTION STEERING COMMITTEE
CONTRIBUTION FORM:
Working Group:       CSCN                        Date of Submission:  2026-02-23
Contribution #:  316C
TIF #:    118                                  File ID:  CNCO316C
Task Title:  Update CSCN-Administered Guidelines for Thousands-Block Pooling
Related to Task(s) ID:  117, 119, 120, 125, 126
Contributor:
            Name:		CNA
            Company:	CNA
            Address:
            Tel:
            Fax:
            E-mail:	david.comrie@cnac.ca
Distribution to:	CSCN
Subject:	Draft Part 1B form for Pooled CO Code and Block requests






NPAC Thousands-Block Data - Part 1B

Revised: January 21, 2025

NPAC Block Holder Data

Submit one form per Thousands-Block.

Block Creation/Activation Request: ☐		Modification Request: ☐

This form should be filled out by applicants who are activating/modifying a new Block where they are not the Code Holder, or where they are the Code Holder but the Block is being allocated to a different LRN.

For Block Creations using NPAC Activation, fill section A and optionally section B.
For activations using SOA Activation, only fill in section A.

Modifications through the CNA can only be done if the application (Part 1A and Part 1B) is submitted 19 calendar days before the NPAC Block Effective Date. Changes on/after the NPAC Block Effective Date must be done by the Block Holder using their SOA or LTI.



Section A:



CNA Contact 

Phone: 613-702-0016

E-Mail: COCodeApps@cnac.ca 



Block Applicant 

Company Name: Click here to enter text.

Contact Name: Click here to enter text.

Address: Click here to enter text.

City:  Click here to enter text.  State: Click here to enter text.  Postal Code: Click here to enter text.

Phone: Click here to enter text. 	

E-Mail: Click here to enter text.  	

Service Provider NPAC SOA SPID[footnoteRef:1]:              Click here to enter text. [1:  The Service Provider ID of the Thousands-Block Holder.  The SPID shall be a valid SPID in the NPAC system. If your company does not have a SPID, please call the NPAC Help Desk for assistance.] 






LRN[footnoteRef:2]:	         Click here to enter text. [2:  A Location Routing Number is a 10-digit number, in the format NPA-NXX-XXXX, that uniquely identifies a Switching Entity/POI.  The NPA-NXX portion of the LRN is used to route calls. ] 




Block (1K) Range[footnoteRef:3]:           Click here to enter text. [3:  The Thousands-Block shall consist of NPA-NXX and the first digit of the 1K block in the format NPA-NXX-X.] 


If Block Applicant is seeking to activate a Thousands-Block, Pooling Administratorthe CNA will fill in the information for the assigned block in the field belowabove. Otherwise for a Modification Request or an Intra SP Block Port Request, Block Holder must specify the Block (1K) Range.



NPAC Block Effective Date: Click here to enter a date.[footnoteRef:4]:       [4:  Typically the NPAC Block Effective Date and the BIRRDS Block Effective Date are the same date. However, based on events in CNAS, BIRRDS or NPAC, the dates may end up different.] 


NPAC Block Effective Date must be equal to or greater than the earliest date that the NPAC shall broadcast the Thousands-Block information to all Local SMSs. If the EffectiveNPAC Block Effective Date Date is blank or the interval too short, the Pooling AdministratorCNA shall set the EffectiveNPAC Block Effective Date Date to the earliest date that the NPAC shall broadcast the Thousands-Block information to all Local SMSs.



Is Block being allocated back to Code Holder on switch whereusing the NXX Code Residessame LRN? Yes☐ No ☐

If “Yes”, Pooling Administratorthe CNA will not send the Part 1B to the NPAC. If “No”, Pooling Administratorthe CNA will forward the Part 1B to the NPAC.



NPAC ActivateActivation of Block Range? Yes ☐	No ☐ (Must Select only One)

NPAC Activation ☐	

SOA Activation ☐

If “YESNPAC” is marked selected the NPAC shall activate the Thousands-Block range. If “NOSOA” is marked selected it shall be the responsibility of the Service Provider (SP) to activate the Thousands-Block range via their Service Order Administration (SOA) system.




Section B:

Block Applicant to provide this data ONLY if NPAC Activate Block Range is marked “Yes.” For Intra SP Block Porting the Thousands-Block Holder should reflect the routing information of the Switching Entity/Point of Interconnection (POI) the Thousands-Block is being transferred to.Activation is selected. 



Whenever a Destination Point Code (DPC) value is specified, a Services Subsystem Number (SSN) value likewise must be provided (and vice versa). 



The format of the DPC shall consist of three 3-digit segments (Network Identification-Network Cluster-Cluster Member) based on the ANSI standard where each segment must be between 000 and 255.  Example: 0-0-0 to 255-255-255.  Signaling Services Subsystem Number (SSN) shall be a value between 0 and 255.



Class DPC[footnoteRef:5]: Click here to enter text. [5:  Customer Local Area Signaling Services Destination Point Code for 10-digit GTT for CLASS features for the 1K block.] 


Class SSN[footnoteRef:6]: Click here to enter text. [6:  Customer Local Area Signaling Services Subsystem Number for the 1K block.] 


LIDB DPC[footnoteRef:7]: Click here to enter text. [7:  Line Information Database Destination Point Code for 10-digit GTT for LIDB features for the 1K block.] 


LIDB SSN[footnoteRef:8]: Click here to enter text. [8:  Line information Database Subsystem Number for the 1K block.] 


CNAM DPC[footnoteRef:9]: Click here to enter text. [9:  Calling Name Delivery Destination Point Code for 10-digit GTT for CNAM features for the 1K block.] 


CNAM SSN[footnoteRef:10]: Click here to enter text. [10:  Calling Name Delivery Subsystem Number for the 1K block.] 


ISVM DPC[footnoteRef:11]: Click here to enter text. [11:  Inter-Switch Voice Mail Destination Point Code for 10-digit GTT for ISVM features for the 1K block.] 


ISVM SSN[footnoteRef:12]: Click here to enter text. [12:  Inter-Switch Voice Mail Services Subsystem Number for the 1K block.] 


WSMSC DPC[footnoteRef:13]: Click here to enter text. [13:  Wireless Short Message Service Center Destination Point Code for 10-digit GTT for WSMSC features.  This field is only required if the Service Provider (SP) supports WSMSC data.] 


WSMSC SSN[footnoteRef:14]: Click here to enter text. [14:  Wireless Short Message Service Center Subsystem Number for the 1K block.  This field is only required if the Service Provider (SP) supports WSMSC data.] 


SOA Origination[footnoteRef:15]: Yes ☐	No ☐
 [15: ] 


Section C:

This section is completed by the NPAC after processing. NPAC is to Activate/Modify/Port the Block (1K), as indicated on this form. When the Block (1K) Activation/Modification is complete, NPAC sends a copy of the completed form to the Pooling AdministratorCNA.

Block (1K) Request Complete: Yes ☐	No ☐

Complete Date: Click here to enter a date.

Complete Time (HH/MM): Click here to enter text.

NPAC Personnel performing change: Click here to enter text.



Block Holder sent Completed Form: Yes ☐	No ☐

Mailed Date: Click here to enter a date.

Mailed Time (HH/MM): Click here to enter text. 

Contact Name: Click here to enter text.

Pooling Administrator sent Completed Form: Yes ☐	No ☐

Mailed Date:  Click here to enter a date.

Mailed Time (HH/MM): Click here to enter text. 

Contact Name: Click here to enter text.



Remarks: Click here to enter text.
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